{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["Chart1","Sheet1","Page 1","Sheet2","Sheet3","Sheet4"],"not_rendered":{"charts":2,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Chart1","index":0,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Page 1","index":2,"n_rows":19,"n_cols":19,"rows_kept":19,"cut":false,"hidden":false,"merged":[[4,4,4,5],[5,1,5,6],[5,7,5,12]]}
[null,"PROCESS FAILURE MODE AND EFFECTS ANALYSIS"]
[]
[null,"Part or Process Name",null,null,null,null,null,"Manufactured By",null,null,null,null,null,"FMEA Date"]
[null,"Laser Cutting",null,null,"FM005",null,null,"Jemison Metals",null,null,null,null,null,"2017-09-14"]
[null,"Core Team",null,null,null,null,null,"Prepared By:"," ",null,null,null,null,"Revision Date/ Revision Level"]
[null,"Rick Rowland, Brian Smith, Bradley Wright, John Foster",null,null,null,null,null,"Rick Rowland",null,null,null,null,null,"2017-09-14",0]
[null,"#","Process\nFunction\nRequirements","Potential\nFailure\nMode","Potential\nEffects of\nFailure","Sev","Class","Potential Cause(s)\nMechanism(s) of\nFailure","Occ","Current\nProcess\nControls","Det","RPN","Recommended\nAction(s)","Responsibility\n& Target Date","Actions\nTaken","Sev","Occ","Det","RPN"]
[]
[null,1,"Enter Program into Machine","Incorrect Program Number","Wrong Parts Cut",8,null,"Typo",3,"First Piece Checks + Nest Layout Provided",1,24]
[null,2,"Correct Material Loaded onto Machine","Wrong Material Loaded","Customer Reject and/or Scrap",8,null,"Mis-Tagged Material, Read the tag incorrectly",3,"Tag # is on work order for verification + 1st Piece Checks",1,24]
[null,2,"Material Thickness","Wrong Material Loaded","Customer Reject and/or Scrap",8,null,"Mis-Tagged Material, Read the tag incorrectly",3,"Laser procedure requires check of Material + 1st piece checks",1,24]
[null,2,"Material Width","Wrong Material Loaded","Excess scrap or not enough parts",6,null,"Mis-Tagged Material, Read the tag incorrectly",3,"Laser procedure requires check of Material + 1st piece checks",1,18]
[null,2,"Material Length","Wrong Material Loaded","Excess scrap or not enough parts",6,null,"Mis-Tagged Material, Read the tag incorrectly",3,"Laser procedure requires check of Material + 1st piece checks",1,18]
[null,2,"Surface Quality","Customer Rejection or Poor Cut Quality","Customer Reject and/or Scrap",5,null,"Scratches, pitting, pickle stain, rust, etc",6,"Laser procedure requires check of Material",2,60]
[null,2,"Material Shape","Laser Head Crash","Unplanned down time, forming issues at P.B.",7,null,"Residual Stress, bow, cross bow, edge wave",4,"Visual Inspection",1,28]
[null,3,"Cut Edge Quality","Incomplete cut or burr/slag","Customer Reject, Scrap or Rework",5,null,"Material Surface Quality, Nozzle issues, Improper Gas Pressure",4,"Visual Inspection + 1st piece inspections.",3,60]
[null,4,"Part Dimensions","Laser out of alignment","Customer Reject, Scrap or Rework",8,null,"Laser mechanism damaged",2,"1st piece inspections",1,16]
[null,5,"Packaging Requirements","Wrong Packaging Used","Customer Unable to Unload or Customer Reject",6,null,"Customer packaging requirements not followed",3,"Work order controls, Shipping Visual Inspection",3,36]
[null,6,"Product Identification","Mis-tagged Material","Customer Rejection",8,null,"Operator Error",5,"Work order controls, Shipping Visual Inspection",2,80]

{"sheet":"Sheet2","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet4","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}